SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( cd_363078_hk
	Comment ( verze: 8.10.2006 definice svetel MSTS Bin )
	
	Comment ( ladenie OR )
	Comment ( Vykon nastaven pro stridavou cast = 3060 kW )
        Comment ( Od B57 pridana EDB nereverzni )        
        Comment ( Svetla: Robo )

	Type ( Engine )
	WagonShape ( "cd_363078_hk.s" )
        Freightanim ( cd_363078fg_hk.s 1 1 )
	Size ( 3.00m 4.69m 16.556m )
	CentreOfGravity ( 0m 2.25m 0m )
	Mass ( 87t )
	WheelRadius ( 0.625m )
	InertiaTensor ( Box (3.00m 4.69m 16.556m) )
Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Chain )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 1e7N/m/s )
			Break ( 1.1e8N 2.5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ( 0 )
		Velocity ( 0.01m/s )
	)
	ORTSAdhesion (
        ORTSCurtius_Kniffler ( 7.5 44 0.161 0.7 )
        )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*87kN )
	DerailBufferForce ( 443kN )
	NumWheels ( 4 )
	Friction (
		1070.5N/m/s    -0.10    1.3mph    12.774N/m/s    1.888
		5.1N/rad/s	1	-1rad/s	0N/rad/s	1
	)

comment	( Wagon Brakes )

 	MaxBrakeForce( 88.42kN )
        MaxHandbrakeForce( 7.97kN )
	NumberOfHandbrakeLeverSteps( 10 )

	BrakeEquipmentType( "Graduated_release_triple_valve, Auxilary_reservoir, Handbrake" )
BrakeSystemType( "Air_single_pipe" )
TripleValveRatio( 2.5 )
MaxReleaseRate( 1.8 )
MaxApplicationRate( 3.13 )
MaxAuxilaryChargingRate( 5.19 )
BrakeCylinderPressureForMaxBrakeBrakeForce( 52.59 )
BrakePipeVolume ( 0.51 )
ORTSBrakeShoeFriction (
  			0	0.31
			1	0.30
			2	0.28
			3	0.27
			4	0.26				
			5	0.25
			7	0.24
			8	0.23
			9	0.22
			12	0.21
			14	0.20
			17	0.19
			20	0.18
			24	0.17
			29	0.16
			34	0.15
			40	0.14
			47	0.13
			55	0.12
			66	0.11
			84	0.10
			115	0.09
			160	0.09
	)

Inside (
		PassengerCabinFile ( cd_363078_hk.s )
		PassengerCabinHeadPos ( -1.6 3.0 6.6 )
		RotationLimit ( 40 90 0 )
		StartDirection ( 0 -90 0 )
	)

comment	( Lights )
	Lights ( 28
		Light (
			comment ( Svetelný kuzel dálkový )
			Type ( 1 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFBFFFF )
					Position ( 0 2.59 7.91 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 50 )
				)
			)
		)    
		Light (
			comment ( Svetelný kuzel tlmeny )
			Type ( 1 )
			Conditions (
				Headlight ( 2 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( AAAAAAAA )
					Position ( 0 1 4 )
					Angle ( 15 )
					Transition ( 1 )
					Radius ( 25 )
				)
			)
		)     
comment ( ovladane svetla, predne stanoviste )
               Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.1 2.58 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.1 2.58 7.91 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFEBC5 )
					Position ( 0 2.53 7.92 )
					Azimuth ( 0 0 0 )
                                        Elevation ( -10 -10 -10 )
					Transition ( 1 )
					Radius ( 0.2 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
					Azimuth ( 0.0 0.0 0.0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 2 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 3 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definice svetel pro zadní stanoviste )

		Light (
			comment ( reflektor lavy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( 0.1 2.58 -7.91 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor pravy dialkový )
			Type ( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFFE085 )
					Position ( -0.1 2.58 -7.91 )
                                        Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.5 )
				)
			)
		)
		Light (
			comment ( reflektor tretie svetlo )
			Type ( 0 )
			Conditions (
				Headlight ( 2 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( 90FFE085 )
					Position ( 0 2.53 -7.92 )
					Elevation ( -10 -10 -10 )
					Azimuth ( 180 180 180 )
					Transition ( 1 )
					Radius ( 0.1 )
				)
			)
		)
                Light (
			comment ( prední levé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( prední pravé zapnuté )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 5 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Headlight ( 4 )
				Unit ( 4 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 7.82 )
					Azimuth ( 0 0 0 )
                                        Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                comment ( Definicia svetiel pre posunujuci diel )

		Light (
			comment ( Prední pravé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
                Light (
			comment ( Prední lave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
					Elevation ( 10 10 10 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní levé pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( zadní prave pozicní )
			Type ( 0 )
			Conditions (
				Headlight ( 1 )
                                Unit ( 0 )
				Control ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		
		comment ( Definice svetel pro Loose consist )
                Light	(
			comment( Lave přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Pravé přední poziční - Loose consist )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Levé zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light	(
			comment( Prave zadní poziční - Loose consist)
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Control ( 0 )
				Service ( 1 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle	( 0 )
			States ( 1
				State	(
					Duration ( 0.0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)

		comment ( Definice svetel pro loko ovládanou PC )

		Light (
			comment ( PC prední pravé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( 0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC prední levé )
			Type ( 0 )
			Conditions (
				Headlight ( 0 )
				Unit ( 2 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 1 )
			FadeOut ( 1 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( EEEED15D )
					Position ( -0.73 1.68 7.82 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC zadní levé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( -0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
		Light (
			comment ( PC zadní pravé koncové )
			Type ( 0 )
			Conditions (
				Unit ( 3 )
				Control ( 1 )
				Service ( 2 )
			)
			FadeIn ( 0.5 )
			FadeOut ( 0.5 )
			Cycle ( 0 )
			States ( 1
				State (
					Duration ( 0 )
					LightColour ( FFFF0000 )
					Position ( 0.98 1.68 -7.83 )
                                        Elevation ( 10 10 10 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.6 )
				)
			)
		)
	)
	Sound ( "..\\..\\common.snd\\ORsndX6X\\362engCD.sms" )
)

Engine ( cd_363078_hk
	Wagon ( "cd_363078_hk" )
	Type ( Electric )
	MaxPower ( 3060kW )
	MaxForce ( 285kN )
	MaxContinuousForce ( 176.5kN )
	DieselEngineSpeedOfMaxTractiveEffort	( 59.3km/h )     
	MaxVelocity ( 120km/h )
	MaxCurrent ( 1100A )
	WheelRadius ( 0.608m )
	Sanding ( 40km/h )
	MaxSandingTime ( 600 )
	NumWheels ( 4 )

	AirBrakesAirCompressorPowerRating ( 2 )  
	AirBrakesAirCompressorWattage ( 32000 )
 	AirBrakesMainMaxAirPressure ( 145 )	
 	AirBrakesCompressorRestartPressure ( 116 )  
	AirBrakesMainMinResAirPressure ( 73 )  
	AirBrakesMainResVolume ( 60 )  
	AirBrakesAirUsedPerPoundsOfBrakePipePressure ( 1 )  
	AirBrakesHasLowPressureTest ( 1 )  
	AirBrakesIsCompressorElectricOrMechanical ( 1 )

	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerMaxApplicationRate ( 5 )
	EngineBrakesControllerMaxReleaseRate ( 5 )
	EngineBrakesControllerEmergencyApplicationRate ( 10 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 73 )
	EngineBrakesControllerDirectControlExponent ( 1 )
	EngineBrakesProportionalBrakeLag( 0.8 )

	TrainBrakesControllerMinPressureReduction ( 0 )
TrainBrakesControllerMaxApplicationRate ( 1.7 )
TrainBrakesControllerMaxReleaseRate ( 1.9 )
TrainBrakesControllerMaxQuickReleaseRate ( 3.8 )
TrainBrakesControllerEmergencyApplicationRate ( 10 )
TrainBrakesControllerMinSystemPressure ( 0 )
TrainBrakesControllerMaxSystemPressure ( 73 )
TrainBrakesControllerEmergencyBrakeTimePenalty ( 0 )
	
TrainPipeLeakRate ( 0.033 )
TrainBrakesControllerFullServicePressureDrop ( 73 )

	DynamicBrakesMaximumForce						( 162kN )
	DynamicBrakesResistorCurrentLimit				( 715 )
	DynamicBrakesDelayTimeBeforeEngaging			( 0 )
	DynamicBrakesNumberOfControllerNotches			( 20 )
	DynamicBrakesMaxAirBrakePressure				( 20 )
	DynamicBrakeHasAutoBailOff						( 1 )

	DynamicBrakesMaximumSpeedForFadeOut				( 100 )
	DynamicBrakesMaximumEffectiveSpeed				( 50 )
	DynamicBrakesHigherSpeedCurveExponent			( 1 )
	DynamicBrakesEffectAtMaximumFadeOut				( 2 )
	DynamicBrakesLowerSpeedCurveExponent			( 1 )
	DynamicBrakesCutInSpeed							( 8 )
	DynamicBrakesFadingSpeed						( 8 )
	DynamicBrakesMinUsableSpeed						( 3 )


	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Independent, Train, Dynamic, Handbrake, Blended" )
	BrakeCutsPowerAtBrakeCylinderPressure ( 15 )
	DoesBrakeCutPower ( 0 )

	CabView ( "../../common.cab/cab363cd/cd_363_Os_ACDC.cvf" )

	DoesHornTriggerBell ( 0 )

EmergencyStopMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 0 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	VigilanceMonitor (
		MonitoringDeviceMonitorTimeLimit ( 20 )
		MonitoringDeviceAlarmTimeLimit ( 10 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 0 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 1 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceResetOnZeroSpeed ( 1 )
		MonitoringDeviceResetOnResetButton ( 1 )
	)
	OverspeedMonitor (
		MonitoringDeviceMonitorTimeLimit ( 0 )
		MonitoringDeviceAlarmTimeLimit ( 5 )
		MonitoringDevicePenaltyTimeLimit ( 0 )
		MonitoringDeviceCriticalLevel ( 89.9 )
		MonitoringDeviceResetLevel ( 0 )
		MonitoringDeviceAppliesFullBrake ( 0 )
		MonitoringDeviceAppliesEmergencyBrake ( 0 )
		MonitoringDeviceAppliesCutsPower ( 1 )
		MonitoringDeviceAppliesShutsDownEngine ( 0 )
		MonitoringDeviceAlarmTimeBeforeOverSpeed ( 10 )
		MonitoringDeviceDoesSuppressionReset ( 0 )
		MonitoringDeviceTriggerOnOverspeed ( 90.0 )
		MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
		MonitoringDeviceTriggerOnTrackOverspeedMargin ( 1.39 )
		MonitoringDeviceResetOnZeroSpeed ( 1 ) 
		MonitoringDeviceResetOnResetButton ( 0 )
	)

	EngineControllers (
		AWS ( 0 1 0 )
		BailOffButton 	( 0 1 0 )
		BellToggle 	( 0 1 0 )
		Brake_Dynamic 	( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Engine 	( 0 1 0.1 0
			NumNotches ( 1
				Notch ( 0 1 Dummy )
			)
		)
		Brake_Hand 	( 0 1 0.1 0
			NumNotches ( 0 )
		)
		Brake_Train ( 0 1 0.05 0.8
                NumNotches ( 6
                Notch ( 0 0 TrainBrakesControllerFullQuickReleaseStart )
                Notch ( 0.4 0 TrainBrakesControllerHoldStart )
                Notch ( 0.5 0 TrainBrakesControllerReleaseStart )
                Notch ( 0.6 0 TrainBrakesControllerNeutralhandleOffStart )
                Notch ( 0.8 0 TrainBrakesControllerContinuousServiceStart )
                Notch ( 0.95 0 TrainBrakesControllerEmergencyStart )
                )
                )
		ORTSTractionCharacteristics (   141   13                                       
   throttle (      0   0.27   0.36   0.45   0.55   0.62   0.65   0.73   0.77   0.82   0.91   1.00   )
   table (                                          
      0km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      1km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      2km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      3km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      4km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      5km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      6km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      7km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      8km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      9km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      10km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      11km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      12km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      13km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      14km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      15km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      16km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      17km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      18km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      19km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      20km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      21km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      22km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.48kN   
      23km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.31kN   223.45kN   239.61kN   271.97kN   296.35kN   
      24km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   178.99kN   210.55kN   223.64kN   239.77kN   271.97kN   294.59kN   
      25km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.37kN   210.79kN   223.83kN   239.94kN   271.97kN   292.83kN   
      26km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.51kN   179.76kN   211.03kN   224.01kN   240.11kN   271.97kN   291.07kN   
      27km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.58kN   167.92kN   180.14kN   211.26kN   224.20kN   240.27kN   271.97kN   289.31kN   
      28km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.78kN   168.32kN   180.51kN   211.50kN   224.38kN   240.44kN   271.97kN   287.55kN   
      29km/h   0.00kN   52.88kN   80.65kN   111.71kN   143.98kN   168.71kN   180.88kN   211.73kN   224.57kN   240.60kN   271.97kN   285.78kN   
      30km/h   0.00kN   52.88kN   80.65kN   111.84kN   144.18kN   169.10kN   181.25kN   211.96kN   224.75kN   240.76kN   271.97kN   284.30kN   
      31km/h   0.00kN   52.88kN   80.65kN   111.96kN   144.38kN   169.48kN   181.61kN   212.19kN   224.93kN   240.92kN   271.97kN   282.49kN   
      32km/h   0.00kN   52.88kN   80.65kN   112.08kN   144.57kN   169.86kN   181.97kN   212.42kN   225.11kN   241.09kN   271.97kN   280.68kN   
      33km/h   0.00kN   52.88kN   80.65kN   112.21kN   144.77kN   170.24kN   182.32kN   212.65kN   225.29kN   241.25kN   271.97kN   278.86kN   
      34km/h   0.00kN   52.88kN   80.81kN   112.33kN   144.96kN   170.61kN   182.67kN   212.87kN   225.47kN   241.41kN   271.97kN   277.05kN   
      35km/h   0.00kN   52.88kN   80.97kN   112.45kN   145.15kN   170.97kN   183.02kN   213.10kN   225.65kN   241.57kN   271.97kN   275.24kN   
      36km/h   0.00kN   52.88kN   81.12kN   112.58kN   145.35kN   171.34kN   183.36kN   213.32kN   225.83kN   241.73kN   271.97kN   273.42kN   
      37km/h   0.00kN   52.88kN   81.28kN   112.70kN   145.54kN   171.69kN   183.70kN   213.54kN   226.00kN   241.88kN   271.97kN   272.60kN   
      38km/h   0.00kN   53.09kN   81.44kN   112.82kN   145.73kN   172.05kN   184.04kN   213.76kN   226.18kN   242.04kN   271.01kN   270.64kN   
      39km/h   0.00kN   53.29kN   81.59kN   112.94kN   145.91kN   172.40kN   184.37kN   213.98kN   226.35kN   242.20kN   269.03kN   268.68kN   
      40km/h   0.00kN   53.49kN   81.75kN   113.06kN   146.10kN   172.74kN   184.70kN   214.20kN   226.53kN   242.36kN   267.06kN   266.72kN   
      41km/h   0.00kN   53.69kN   81.90kN   113.18kN   146.29kN   173.09kN   185.02kN   214.41kN   226.70kN   242.51kN   265.08kN   264.76kN   
      42km/h   0.00kN   53.89kN   82.06kN   113.30kN   146.47kN   173.43kN   185.35kN   214.63kN   226.87kN   242.67kN   263.11kN   262.80kN   
      43km/h   0.00kN   54.09kN   82.21kN   113.42kN   146.65kN   173.76kN   185.67kN   214.84kN   227.04kN   242.82kN   261.13kN   260.85kN   
      44km/h   0.00kN   54.28kN   82.36kN   113.54kN   146.84kN   174.09kN   185.98kN   215.05kN   227.22kN   242.98kN   259.16kN   258.89kN   
      45km/h   0.00kN   54.47kN   82.51kN   113.65kN   147.02kN   174.42kN   186.30kN   215.26kN   227.39kN   243.13kN   257.19kN   256.94kN   
      46km/h   0.00kN   54.66kN   82.66kN   113.77kN   147.20kN   174.75kN   186.61kN   215.32kN   227.55kN   243.28kN   255.22kN   254.99kN   
      47km/h   0.00kN   54.85kN   82.81kN   113.89kN   147.38kN   175.07kN   186.91kN   215.32kN   227.72kN   243.43kN   253.25kN   253.04kN   
      48km/h   0.00kN   55.04kN   82.95kN   114.00kN   147.55kN   175.39kN   187.22kN   215.32kN   227.89kN   243.59kN   251.28kN   251.09kN   
      49km/h   0.00kN   55.23kN   83.10kN   114.12kN   147.73kN   175.70kN   187.52kN   215.32kN   228.06kN   243.74kN   249.32kN   249.14kN   
      50km/h   0.00kN   55.41kN   83.25kN   114.23kN   147.91kN   176.01kN   187.82kN   215.32kN   228.22kN   243.89kN   247.35kN   247.19kN   
      51km/h   0.00kN   55.60kN   83.39kN   114.35kN   148.08kN   176.32kN   188.11kN   215.32kN   228.39kN   242.60kN   245.39kN   245.25kN   
      52km/h   0.00kN   55.78kN   83.54kN   114.46kN   148.25kN   176.63kN   188.41kN   215.32kN   228.55kN   240.98kN   243.55kN   243.43kN   
      53km/h   0.00kN   55.96kN   83.68kN   114.58kN   148.43kN   176.93kN   188.70kN   215.32kN   228.72kN   239.37kN   241.57kN   241.46kN   
      54km/h   0.00kN   56.14kN   83.82kN   114.69kN   148.60kN   177.23kN   188.98kN   215.32kN   228.88kN   237.76kN   239.59kN   239.50kN   
      55km/h   0.00kN   56.32kN   83.96kN   114.80kN   148.77kN   177.53kN   189.27kN   215.32kN   229.04kN   236.15kN   237.62kN   237.54kN   
      56km/h   0.00kN   56.49kN   84.10kN   114.91kN   148.94kN   177.82kN   189.55kN   215.32kN   229.21kN   234.54kN   235.64kN   235.59kN   
      57km/h   0.00kN   56.67kN   84.24kN   115.03kN   149.11kN   178.11kN   189.83kN   215.32kN   229.37kN   232.94kN   233.67kN   233.63kN   
      58km/h   0.00kN   56.84kN   84.38kN   115.14kN   149.27kN   178.40kN   190.11kN   215.32kN   229.53kN   231.33kN   231.70kN   231.68kN   
      59km/h   0.00kN   57.01kN   84.52kN   115.25kN   149.44kN   178.68kN   190.38kN   215.32kN   229.69kN   229.72kN   229.72kN   229.72kN   
      60km/h   0.00kN   57.18kN   84.66kN   115.36kN   149.61kN   175.44kN   186.98kN   214.30kN   225.65kN   227.69kN   229.72kN   229.72kN   
      61km/h   0.00kN   57.35kN   84.80kN   115.47kN   149.77kN   172.24kN   183.62kN   210.54kN   221.66kN   223.70kN   226.11kN   226.11kN   
      62km/h   0.00kN   57.52kN   84.93kN   115.58kN   149.93kN   169.08kN   180.29kN   206.82kN   217.70kN   219.75kN   222.17kN   222.17kN   
      63km/h   0.00kN   57.69kN   85.07kN   115.69kN   147.19kN   165.97kN   177.01kN   203.14kN   213.79kN   215.84kN   218.26kN   218.26kN   
      64km/h   0.00kN   57.85kN   85.20kN   115.80kN   144.50kN   162.93kN   173.78kN   199.51kN   209.93kN   211.97kN   214.39kN   214.39kN   
      65km/h   0.00kN   58.02kN   85.34kN   115.90kN   141.86kN   159.95kN   170.62kN   195.92kN   206.14kN   208.17kN   210.57kN   210.57kN   
      66km/h   0.00kN   58.18kN   85.47kN   116.01kN   139.29kN   157.04kN   167.53kN   192.40kN   202.42kN   204.43kN   206.81kN   206.81kN   
      67km/h   0.00kN   58.34kN   85.60kN   113.92kN   136.78kN   154.22kN   164.51kN   188.95kN   198.78kN   200.76kN   203.11kN   203.11kN   
      68km/h   0.00kN   58.50kN   85.74kN   111.90kN   134.35kN   151.49kN   161.58kN   185.58kN   195.23kN   197.17kN   199.49kN   199.49kN   
      69km/h   0.00kN   58.66kN   85.87kN   109.94kN   132.00kN   148.86kN   158.75kN   182.29kN   191.79kN   193.68kN   195.96kN   195.96kN   
      70km/h   0.00kN   58.82kN   86.00kN   108.05kN   129.74kN   146.32kN   156.01kN   179.10kN   188.44kN   190.29kN   192.51kN   192.51kN   
      71km/h   0.00kN   58.97kN   84.54kN   106.23kN   127.57kN   143.89kN   153.37kN   176.01kN   185.21kN   187.01kN   189.17kN   189.17kN   
      72km/h   0.00kN   59.13kN   83.15kN   104.48kN   125.48kN   141.56kN   150.84kN   173.03kN   182.10kN   183.84kN   185.93kN   185.93kN   
      73km/h   0.00kN   59.28kN   81.81kN   102.82kN   123.49kN   139.33kN   148.42kN   170.16kN   179.12kN   180.79kN   182.81kN   182.81kN   
      74km/h   0.00kN   59.43kN   80.54kN   101.22kN   121.59kN   137.21kN   146.11kN   167.40kN   176.25kN   177.86kN   179.80kN   179.80kN   
      75km/h   0.00kN   58.54kN   79.32kN   99.71kN   119.78kN   135.20kN   143.90kN   164.76kN   173.52kN   175.05kN   176.92kN   176.92kN   
      76km/h   0.00kN   57.68kN   78.17kN   98.27kN   118.06kN   133.29kN   141.81kN   162.23kN   170.91kN   172.37kN   174.15kN   174.15kN   
      77km/h   0.00kN   56.87kN   77.07kN   96.90kN   116.44kN   131.49kN   139.82kN   159.83kN   168.42kN   169.82kN   171.51kN   171.51kN   
      78km/h   0.00kN   56.10kN   76.03kN   95.61kN   114.90kN   129.78kN   137.93kN   157.54kN   166.07kN   167.38kN   168.99kN   168.99kN   
      79km/h   0.00kN   55.37kN   75.05kN   94.38kN   113.44kN   128.17kN   136.15kN   155.36kN   163.83kN   165.07kN   166.59kN   166.59kN   
      80km/h   0.00kN   54.69kN   74.13kN   93.23kN   112.07kN   126.66kN   134.47kN   153.30kN   161.71kN   162.88kN   164.31kN   164.31kN   
      81km/h   0.00kN   54.04kN   73.25kN   92.14kN   110.78kN   125.23kN   132.88kN   151.35kN   159.71kN   160.81kN   162.15kN   162.15kN   
      82km/h   0.00kN   53.43kN   72.43kN   91.12kN   109.56kN   123.88kN   131.39kN   149.50kN   157.82kN   158.85kN   160.11kN   160.11kN   
      83km/h   0.00kN   52.85kN   71.65kN   90.16kN   108.42kN   122.62kN   129.98kN   147.76kN   156.04kN   156.99kN   158.17kN   158.17kN   
      84km/h   0.00kN   52.31kN   70.92kN   89.25kN   107.35kN   121.44kN   128.66kN   146.11kN   154.36kN   155.25kN   156.34kN   156.34kN   
      85km/h   0.00kN   51.80kN   70.24kN   88.40kN   106.34kN   120.32kN   127.41kN   144.57kN   152.78kN   153.60kN   154.61kN   154.61kN   
      86km/h   0.00kN   51.32kN   69.59kN   87.60kN   105.39kN   119.28kN   126.25kN   143.11kN   151.29kN   152.05kN   152.99kN   152.99kN   
      87km/h   0.00kN   50.88kN   68.99kN   86.85kN   104.50kN   118.30kN   125.15kN   141.73kN   149.89kN   150.59kN   151.45kN   151.45kN   
      88km/h   0.00kN   50.46kN   68.42kN   86.15kN   103.67kN   117.39kN   124.12kN   140.44kN   148.58kN   149.22kN   150.01kN   150.01kN   
      89km/h   0.00kN   50.06kN   67.89kN   85.49kN   102.89kN   116.53kN   123.16kN   139.23kN   147.35kN   147.93kN   148.65kN   148.65kN   
      90km/h   0.00kN   49.69kN   67.39kN   84.87kN   102.16kN   115.72kN   122.25kN   138.08kN   146.19kN   146.71kN   147.37kN   147.37kN   
      91km/h   0.00kN   49.34kN   66.93kN   84.29kN   101.47kN   114.97kN   121.40kN   137.01kN   145.10kN   145.58kN   146.17kN   146.17kN   
      92km/h   0.00kN   49.02kN   66.49kN   83.75kN   100.83kN   114.27kN   120.61kN   136.01kN   144.08kN   144.51kN   145.04kN   145.04kN   
      93km/h   0.00kN   48.71kN   66.08kN   83.24kN   100.23kN   113.61kN   119.86kN   135.06kN   143.12kN   143.50kN   143.97kN   143.97kN   
      94km/h   0.00kN   48.43kN   65.69kN   82.76kN   99.66kN   112.99kN   119.16kN   134.17kN   142.22kN   142.56kN   142.98kN   142.98kN   
      95km/h   0.00kN   48.16kN   65.33kN   82.32kN   99.13kN   112.41kN   118.51kN   133.34kN   141.38kN   141.67kN   142.04kN   142.04kN   
      96km/h   0.00kN   47.91kN   64.99kN   81.90kN   98.64kN   111.86kN   117.89kN   132.56kN   140.59kN   140.84kN   141.16kN   141.16kN   
      97km/h   0.00kN   47.67kN   64.67kN   81.50kN   98.17kN   111.35kN   117.32kN   131.82kN   139.85kN   140.06kN   140.33kN   140.33kN   
      98km/h   0.00kN   47.45kN   64.38kN   81.13kN   97.74kN   110.88kN   116.78kN   131.13kN   139.15kN   139.33kN   139.55kN   139.55kN   
      99km/h   0.00kN   47.24kN   64.10kN   80.79kN   97.33kN   110.43kN   116.27kN   130.48kN   138.49kN   138.64kN   138.82kN   138.82kN   
      100km/h   0.00kN   47.05kN   63.83kN   80.46kN   96.95kN   110.01kN   115.80kN   129.88kN   137.88kN   137.99kN   138.13kN   138.13kN   
      101km/h   0.00kN   46.87kN   63.59kN   80.16kN   96.59kN   109.62kN   115.35kN   129.30kN   137.30kN   137.39kN   137.49kN   137.49kN   
      102km/h   0.00kN   46.70kN   63.36kN   79.88kN   96.25kN   109.25kN   114.93kN   128.77kN   136.76kN   136.82kN   136.88kN   136.88kN   
      103km/h   0.00kN   46.53kN   63.14kN   79.61kN   95.93kN   108.90kN   114.54kN   128.26kN   136.25kN   136.28kN   136.31kN   136.31kN   
      104km/h   0.00kN   46.38kN   62.94kN   79.36kN   95.64kN   108.57kN   114.17kN   127.79kN   135.78kN   135.78kN   135.78kN   135.78kN   
      105km/h   0.00kN   46.09kN   62.54kN   78.86kN   95.04kN   107.89kN   113.45kN   126.99kN   133.59kN   133.59kN   133.59kN   133.59kN   
      106km/h   0.00kN   45.80kN   62.14kN   78.35kN   94.43kN   107.20kN   112.73kN   126.18kN   131.41kN   131.41kN   131.41kN   131.41kN   
      107km/h   0.00kN   45.50kN   61.74kN   77.85kN   93.82kN   106.51kN   112.00kN   125.36kN   129.24kN   129.24kN   129.24kN   129.24kN   
      108km/h   0.00kN   45.20kN   61.33kN   77.33kN   93.20kN   105.81kN   111.26kN   124.53kN   127.09kN   127.09kN   127.09kN   127.09kN   
      109km/h   0.00kN   44.90kN   60.92kN   76.81kN   92.57kN   105.10kN   110.51kN   123.70kN   124.94kN   124.94kN   124.94kN   124.94kN   
      110km/h   0.00kN   44.59kN   60.51kN   76.29kN   91.94kN   104.38kN   109.76kN   122.86kN   122.86kN   122.86kN   122.86kN   122.86kN   
      111km/h   0.00kN   44.28kN   60.09kN   75.76kN   91.31kN   103.66kN   109.00kN   120.72kN   120.72kN   120.72kN   120.72kN   120.72kN   
      112km/h   0.00kN   43.97kN   59.67kN   75.23kN   90.66kN   102.93kN   108.23kN   118.58kN   118.58kN   118.58kN   118.58kN   118.58kN   
      113km/h   0.00kN   43.66kN   59.24kN   74.69kN   90.01kN   102.19kN   107.46kN   116.46kN   116.46kN   116.46kN   116.46kN   116.46kN   
      114km/h   0.00kN   43.34kN   58.81kN   74.15kN   89.36kN   101.45kN   106.67kN   114.35kN   114.35kN   114.35kN   114.35kN   114.35kN   
      115km/h   0.00kN   43.02kN   58.37kN   73.60kN   88.70kN   100.69kN   105.88kN   112.25kN   112.25kN   112.25kN   112.25kN   112.25kN   
      116km/h   0.00kN   42.69kN   57.93kN   73.04kN   88.03kN   99.94kN   105.08kN   110.15kN   110.15kN   110.15kN   110.15kN   110.15kN   
      117km/h   0.00kN   42.37kN   57.49kN   72.48kN   87.35kN   99.17kN   104.28kN   108.07kN   108.07kN   108.07kN   108.07kN   108.07kN   
      118km/h   0.00kN   42.03kN   57.04kN   71.92kN   86.67kN   98.39kN   103.46kN   106.00kN   106.00kN   106.00kN   106.00kN   106.00kN   
      119km/h   0.00kN   41.70kN   56.58kN   71.34kN   85.98kN   97.61kN   102.64kN   103.95kN   103.95kN   103.95kN   103.95kN   103.95kN   
      120km/h   0.00kN   41.36kN   56.13kN   70.77kN   85.29kN   96.82kN   101.81kN   101.90kN   101.90kN   101.90kN   101.90kN   101.90kN   
      121km/h   0.00kN   41.02kN   55.66kN   70.18kN   84.58kN   96.02kN   99.87kN   99.87kN   99.87kN   99.87kN   99.87kN   99.87kN   
      122km/h   0.00kN   40.68kN   55.20kN   69.59kN   83.87kN   95.22kN   97.90kN   97.90kN   97.90kN   97.90kN   97.90kN   97.90kN   
      123km/h   0.00kN   40.33kN   54.72kN   69.00kN   83.16kN   94.41kN   95.88kN   95.88kN   95.88kN   95.88kN   95.88kN   95.88kN   
      124km/h   0.00kN   39.98kN   54.25kN   68.40kN   82.43kN   93.58kN   93.87kN   93.87kN   93.87kN   93.87kN   93.87kN   93.87kN   
      125km/h   0.00kN   39.63kN   53.77kN   67.79kN   81.70kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   91.87kN   
      126km/h   0.00kN   39.27kN   53.28kN   67.18kN   80.97kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   89.89kN   
      127km/h   0.00kN   38.91kN   52.79kN   66.56kN   80.22kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   87.93kN   
      128km/h   0.00kN   38.54kN   52.30kN   65.94kN   79.47kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   86.06kN   
      129km/h   0.00kN   38.17kN   51.80kN   65.31kN   78.71kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   84.11kN   
      130km/h   0.00kN   37.80kN   51.29kN   64.67kN   77.94kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   82.16kN   
      131km/h   0.00kN   37.43kN   50.78kN   64.03kN   77.17kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   80.24kN   
      132km/h   0.00kN   37.05kN   50.27kN   63.38kN   76.39kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   78.33kN   
      133km/h   0.00kN   36.66kN   49.75kN   62.73kN   75.60kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   76.43kN   
      134km/h   0.00kN   36.28kN   49.23kN   62.07kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   74.55kN   
      135km/h   0.00kN   35.89kN   48.70kN   61.40kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   72.69kN   
      136km/h   0.00kN   35.50kN   48.16kN   60.73kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   70.84kN   
      137km/h   0.00kN   35.10kN   47.62kN   60.05kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   69.01kN   
      138km/h   0.00kN   34.70kN   47.08kN   59.36kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   67.20kN   
      139km/h   0.00kN   34.29kN   46.53kN   58.67kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   65.40kN   
      140km/h   0.00kN   33.88kN   45.98kN   57.97kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   63.69kN   
   )                                          
)
		Throttle 	( 0 1 0.05 0
			NumNotches ( 0 )
		)
		DirControl 		( -1 0 1 1 )
		EmergencyStopToggle	( 0 1 0 )
		Headlights 		( 0 0.5 1 0 )
		Horn 			( 0 1 0 )
		PantographToggle1 ( 0 1 0 )
		PantographToggle2 ( 0 1 0 )
		PantographsToggle_4 ( 0 1 0 )
		Sanding 		( 0 1 0 )
		Vigilance 		( 0 1 0 )
		Wipers 			( 0 1 0 )
	)

	Name ( "CD 363 078-3 HK-ZOO" )
	Sound ( "..\\..\\common.snd\\ORsndX6X\\362cabCD.sms" )

	Description (
		"Rada 362 CD je univerzalni elektricka skrinova lokomotiva, pouzivana v osobni a nákladní doprave.\nTyp Bo'-Bo', napeti 3kV ss , 25kV 50Hz str.\n\nDelka pres narazniky: 16,8 m\n\nPrumer hnacich kol: 1250 mm\n\nHmotnost ve sluzbe: 87 t\n\n" +
		"Trvaly vykon trakcnich motoru: 3480 kW ss , 3060kW str.\n\n" +
		"Max. rychlost 140 km/h\n" +
		""
	)
)
